.Language=English,English
.PluginContents=SEFP2


@Contents
$ #SEFP2 version 1.2.0.145#
System requirements: Win2K+ / FAR 2.0.1420+

  ~What is SEFP2~@hcWhatIs@

  ~Configure plugin~@hcConfigure@

  ~Supported Phones~@hcSupportedPhones@

  ~Connecting a phone~@hcConnect@

  ~Working with a phone~@hcWork@


Visit us: #www.davinciteam.com#

@hcWhatIs
$ #SEFP2 - What is PhoneFS#
  #SEFP2# brings all the power of #Far  Manager#  to  SEMC mobile phone's
internal filesystem. SEFP2 uses native SEMC protocol to access files. You can work with folders
as easy as with single file. SEFP2 recursively process all files insidea folder. 
On a progress screen during the process You can see:


   -#Source and Destanation filenames#

   -#Current file progress bar#

   -#Total files size information#

   -#Total progress bar#

   -#Number of files processed/total#

   -#Time elapsed and estimate#

   -#Current transfer speed#




  ~Go to main screen~@Contents@

@hcConfigure
$ #SEFP2 - Configure plugin#
  Before the beginning of work with SEFP2, You need to adjust  some
parameters. To enter in the configuration menu, choose #SEFP2# from
the Far menu #Options#/#Plugins configuration#:


   #Add to Plugins menu#         - leave checked if You want to  see 
PhoneFS in Plugins dialog #F11#

   #Add to Disks menu#           - leave checked to be able to select
PhoneFS from Disks menu #Alt+F1/Alt+F2#

   #Disks menu hotkey ('1'-'9')# - set desired hotkey for Disks menu.
Leave blank for autoassign



 
  ~Go to main screen~@Contents@

@hcSupportedPhones
$ #SEFP2 - Supported phones#
  #SEFP2# working with next models: 

 ~SEMC A1~
 #DB2010 CID36/49 RED/BROWN:#
 D750,K310,K510,K750,K758,W300,W550,W600,W700,W800,
 W810,Z520,Z525,Z530,Z550,Z558
 #DB2012 CID50/53 RED/BROWN:#
 K310,K320,K510,W200,W300,W810,Z550
 #DB2020 CID49/51/52/53 RED/BROWN:#
 K530,K550,K610,K618,K770,K790,K800,K810,S500,T650,V630,
W580,W610,W660,W710,W830,W850,W880,Z610,Z710
 #PNX5230 CID49/51/52/53 RED/BROWN:#
 W350,W380,Z310,Z555

 ~SEMC A2~
 #DB3150 CID49/51/52 RED/BROWN/BLUE:#
 C702,C902,G502,K630,K660,K850,K858,T700,TM506,V640,W595,
W760,W890,W902,W908,W910,W980,Z750,Z770,Z780
 #DB3200 CID49/51/52/53/80/81 RED/BROWN/BLUE:#
 F100,J105,T707,TM717,W508,W518
 #DB3210 CID49/51/52/53/80/81 RED/BROWN/BLUE:#
 C510,C901,C903,C905,G705,TM715,W705,W715,W995
 #DB3350 CID49/51/52/53/80/81 RED/BROWN/BLUE:#
 J10,J20,U10,U100,W20,X5



  ~Go to main screen~@Contents@

@hcSupportedActions
$ #SEFP2 - Actions available table#

 ------------------------------------------------------------------
 Domain |        RED            |       BROWN            | SUPERCID
 ------------------------------------------------------------------
 CID    |36 49 50 51 52 53 80 81| 36 49 50 51 52 53 80 81|   ANY
 ------------------------------------------------------------------
 DB2010 |WO WO -- -- -- -- -- --| RW RW -- -- -- -- -- --|   RW
 DB2012 |-- -- WO WO WO WO -- --| -- -- RW RW -- -- -- --|   RW
 DB2020 |-- WO -- WO WO WO -- --| RW RW -- -- -- -- -- --|   RW
 PNX5230|-- -- -- WO WO WO -- --| -- RW -- RW RW -- -- --|   --
 DB3150 |-- RW -- RW RW -- -- --| -- RW -- RW RW -- -- --|   RW
 DB3200 |-- RW -- RW RW WO WO WO| -- RW -- RW RW RW RW RW|   RW
 DB3210 |-- RW -- RW RW WO WO WO| -- RW -- RW RW RW RW RW|   RW
 DB3350 |-- RW -- RW RW WO WO WO| -- RW -- RW RW RW RW RW|   RW
-------------------------------------------------------------------

 RW - Reading, writing and access attributes available
 WO - Writing only available
 -- - Not exists / not supported
 Files and folders delete supported in any CID/Color combination

 RED      - Retail product (PRODUCT)
 BROWN    - Developer device (R&D)
 BLUE     - Factory device (FACTORY)
 SUPERCID - Security disabled device. Any color



  ~Go to main screen~@Contents@

@hcWork
$ #SEFP2 - Working with a phone#
  SEFP2 allows You to work with a phone filesystem absolutely the same way
as You doing it with a local drive:


  #F5#/#F6#          - Copy/move a file/folder from/to the local disk.

  #F7#             - Create a new folder on a phone.

  #F8#             - Delete file/folder from a phone.

  #Alt+F7#         - Find files




  ~Go to main screen~@Contents@

@hcConnect
$ #SEFP2 - Connecting a phone#
   You can open SEFP2 from Disks Menu #Alt+F1#/#Alt+F2# or from Plugins
Dialog #F11#. No additional software (PC Suite etc.) required for SEFP2 
to work. You need to have USB flashing cable drivers only.


  ~SonyEricsson~

   Before connect the phone You need to make sure battery is fully charged, 
otherwise You can lose some data.
Phone can be connected by USB cable. #DCU-60# / #DCU-65# is the cable that comes 
with phone in a box. Drivers You can find in Download Area at #www.davinciteam.com# 
To connect a phone You need:
-Power OFF the phone and reinsert battery
-Open SEFP2 start dialog and press Connect
-Connect USB cable holding #C# button






  ~Go to main screen~@Contents@
@hcCopy
$ #SEFP2 - Copy#
   Specify destenation path for files to place



  ~Go to main screen~@Contents@

@hcMakeDirectory
$ #SEFP2 - Make Directory#
   Specify the new folder name



  ~Go to main screen~@Contents@

@hcDelete
$ #SEFP2 - Delete#
   Confirm files delete from a phone



  ~Go to main screen~@Contents@

@hcA1FilesystemErrors
$ #SEFP2 - A1 filesystem error codes#
   0x01 - Unknown error
   0x02 - File, directory or volume not found
   0x03 - Not enough free space on volume to perform operation
   0x04 - The access permission attributes do not allow operation
   0x05 - Specified path does not point to a directory
   0x06 - There already exists a named file with given name
   0x07 - Signed file archive error
   0x08 - Not authenticated / Not supported
   0x09 - File system is formatting



  ~Go to main screen~@Contents@

@hcA2FilesystemErrors
$ #SEFP2 - A2 filesystem error codes#
   0x01 - The loader does not support the property
   0x02 - The property is read only
   0x03 - The property value is invalid
   0x04 - The access permission attributes do not allow operation
   0x05 - The file system is busy formatting
   0x06 - The path does not exist
   0x07 - The path already exists
   0x08 - The path is read only
   0x09 - Insufficient space
   0x0A - The directory is not empty
   0x0B - The specified access restriction is invalid
   0x0C - Could not find any file system configuration from the platform software in the flash
   0x0D - The file does not exist
   0x0E - Failed to change directory
   0x0F - Failed to set new CH mod
   0x10 - Failed to get the current directory
   0x11 - Failed to open a file in the file system
   0x12 - Failed to read the stat from file
   0x13 - Failed to list volumes
   0x14 - No free space left
   0x15 - Failed to close a file in the file system
   0x16 - Failed to close the directory
   0x17 - Failed to remove a file from the file system
   0x18 - Failed to rename a file in the file system
   0x19 - Failed to create a new directory in the file system
   0x1A - Failed to remove a directory from the file system
   0x1B - Failed to write a file to the file system
   0x1C - The state of the SFA programming is incorrect



  ~Go to main screen~@Contents@
